<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.40.13-Bratislava">
  <identifier>C:\Job\2026\QGIS SHA Project using the USLE Lake Baikal case study\external_data\MI_GEM2023_1T50P10.gpkg|layername=viii_t50p10</identifier>
  <parentidentifier></parentidentifier>
  <language>eng (English)</language>
  <type>dataset</type>
  <title>GEM Global SEISMIC HAZARD MAP v 2023.1 macroseismic intensity VIII+ map for the Lake Baikal region for 10% probability of exceedance in 50 years</title>
  <abstract>GEM Global SEISMIC HAZARD MAP v 2023.1 
Copyright (C) 2023 GEM Foundation 
Macroseismic intensity fields for intensity classes VIII+ or larger for the Lake Baikal region for 10% probability of exceedance in 50 year.
I(PGA)=2.5×log10(PGA)+1.89 (GOST R 57546-2017)
GOST R 57546-2017 National Standard of the Russian Federation. Earthquakes. Scale of seismic intensity. Date of introduction 2017-09-01 (in Russian)</abstract>
  <keywords vocabulary="GIS">
    <keyword>geospatial</keyword>
  </keywords>
  <keywords vocabulary="PSHA Concept">
    <keyword>GEM Global SEISMIC HAZARD MAP v 2023.1</keyword>
  </keywords>
  <keywords vocabulary="Seismic Hazard">
    <keyword>macroseismic intensity</keyword>
  </keywords>
  <keywords vocabulary="geographicRegion">
    <keyword>Lake Baikal region</keyword>
  </keywords>
  <keywords vocabulary="gmd:topicCategory">
    <keyword>Geoscientific Information</keyword>
    <keyword>Seismic Hazard</keyword>
  </keywords>
  <contact>
    <name>Anastasiia Nekrasova</name>
    <organization>Institute of Earthquake Prediction Theory and Mathematical Geophysics RAS</organization>
    <position></position>
    <voice></voice>
    <fax></fax>
    <email>nastia$mitp.ru</email>
    <role>owner</role>
  </contact>
  <links>
    <link type="information" size="" name="Interactive Geographic Information Projects" format="" url="https://www.itpz-ran.ru/en/results/maps-and-databases/" description="" mimeType=""/>
  </links>
  <history></history>
  <dates/>
  <fees></fees>
  <constraints type="undefined 1">No restrictions for academic use. For citation, reference: Pagani M, Garcia-Pelaez J, Gee R, et al. The 2018 version of the Global Earthquake Model: Hazard component. Earthquake Spectra. 2020; 36(1_suppl):226-251. doi:10.1177/8755293020931866
</constraints>
  <license>Project Draft License 1.0 (Placeholder)</license>
  <encoding></encoding>
  <crs>
    <spatialrefsys nativeFormat="Wkt">
      <wkt>PROJCRS["WGS 84 / Pseudo-Mercator",BASEGEOGCRS["WGS 84",ENSEMBLE["World Geodetic System 1984 ensemble",MEMBER["World Geodetic System 1984 (Transit)"],MEMBER["World Geodetic System 1984 (G730)"],MEMBER["World Geodetic System 1984 (G873)"],MEMBER["World Geodetic System 1984 (G1150)"],MEMBER["World Geodetic System 1984 (G1674)"],MEMBER["World Geodetic System 1984 (G1762)"],MEMBER["World Geodetic System 1984 (G2139)"],MEMBER["World Geodetic System 1984 (G2296)"],ELLIPSOID["WGS 84",6378137,298.257223563,LENGTHUNIT["metre",1]],ENSEMBLEACCURACY[2.0]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],ID["EPSG",4326]],CONVERSION["Popular Visualisation Pseudo-Mercator",METHOD["Popular Visualisation Pseudo Mercator",ID["EPSG",1024]],PARAMETER["Latitude of natural origin",0,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8801]],PARAMETER["Longitude of natural origin",0,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8802]],PARAMETER["False easting",0,LENGTHUNIT["metre",1],ID["EPSG",8806]],PARAMETER["False northing",0,LENGTHUNIT["metre",1],ID["EPSG",8807]]],CS[Cartesian,2],AXIS["easting (X)",east,ORDER[1],LENGTHUNIT["metre",1]],AXIS["northing (Y)",north,ORDER[2],LENGTHUNIT["metre",1]],USAGE[SCOPE["Web mapping and visualisation."],AREA["World between 85.06°S and 85.06°N."],BBOX[-85.06,-180,85.06,180]],ID["EPSG",3857]]</wkt>
      <proj4>+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs</proj4>
      <srsid>3857</srsid>
      <srid>3857</srid>
      <authid>EPSG:3857</authid>
      <description>WGS 84 / Pseudo-Mercator</description>
      <projectionacronym>merc</projectionacronym>
      <ellipsoidacronym>EPSG:7030</ellipsoidacronym>
      <geographicflag>false</geographicflag>
    </spatialrefsys>
  </crs>
  <extent>
    <spatial minz="0" minx="11020629.5885000005364418" miny="6106854.83490000013262033" maxz="0" dimensions="2" maxy="7967317.53500000014901161" crs="EPSG:3857" maxx="13580977.87680000066757202"/>
    <temporal>
      <period>
        <start></start>
        <end></end>
      </period>
    </temporal>
  </extent>
</qgis>
