<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.40.13-Bratislava">
  <identifier>C:\Job\2026\QGIS SHA Project using the USLE Lake Baikal case study\data\MCM_USLE_structural_dominant_directions.gpkg|layername=MCM_USLE_structural_dominant_directions_t50p10</identifier>
  <parentidentifier></parentidentifier>
  <language>eng (English)</language>
  <type>dataset</type>
  <title>Maximum Credible Magnitude T50P10 structural dominant_directions (USLE regional coefficients, BDRGS catalog data 1994-2019)</title>
  <abstract>Identification of potential seismic sources 
The primary impact direction is defined as the dominant strike of the regional active fault system. The directions were derived from the AFEAD_v2022_BKL database and represent the prevailing orientations of seismogenic structures as constrained by the maximum expected earthquake magnitudes within the USLE framework. T
he methodological background and the QGIS plugin used for constructing the dominant fault directions are described in Emelyanov I.V. and Nekrasova A.K. (2022). 
Emelyanov I.V., Nekrasova A.K. (2022) DDLAFS — QGIS plugin for dominant directions of the local active fault system estimation.Geoinformatika. (4):54–62. https://doi.org/10.47148/1609-364X-2022-4-54-62. In Russian.</abstract>
  <keywords vocabulary="NDSHA concept">
    <keyword>Neo-Deterministic Seismic Hazard Assessment</keyword>
  </keywords>
  <keywords vocabulary="geographicRegion">
    <keyword>Lake Baikal region</keyword>
  </keywords>
  <keywords vocabulary="gmd:topicCategory">
    <keyword>Geoscientific Information</keyword>
    <keyword>Seismic Hazard</keyword>
  </keywords>
  <keywords vocabulary="seismichazard">
    <keyword>seismic hazard</keyword>
  </keywords>
  <contact>
    <name>Anastasiia Nekrasova</name>
    <organization>Institute of Earthquake Prediction Theory and Mathematical Geophysics RAS</organization>
    <position></position>
    <voice></voice>
    <fax></fax>
    <email>nastia$mitp.ru</email>
    <role>owner</role>
  </contact>
  <links>
    <link type="information" size="" mimeType="" url="https://www.itpz-ran.ru/en/results/maps-and-databases/" description="" format="" name="Interactive Geographic Information Projects"/>
  </links>
  <history></history>
  <dates/>
  <fees></fees>
  <constraints type="undefined 1">No restrictions for academic use. For citation, reference the Nekrasova, A., Kossobokov, V. (2023) Seismic risk assessment for the infrastructure in the regions adjacent to the Russian Federation Baikal–Amur Mainline based on the Unified Scaling Law for Earthquakes. Nat Hazards 116, 2. https://doi.org/10.1007/s11069-022-05750-9</constraints>
  <license>Project Draft License 1.0 (Placeholder)</license>
  <encoding></encoding>
  <crs>
    <spatialrefsys nativeFormat="Wkt">
      <wkt>GEOGCRS["WGS 84",ENSEMBLE["World Geodetic System 1984 ensemble",MEMBER["World Geodetic System 1984 (Transit)"],MEMBER["World Geodetic System 1984 (G730)"],MEMBER["World Geodetic System 1984 (G873)"],MEMBER["World Geodetic System 1984 (G1150)"],MEMBER["World Geodetic System 1984 (G1674)"],MEMBER["World Geodetic System 1984 (G1762)"],MEMBER["World Geodetic System 1984 (G2139)"],MEMBER["World Geodetic System 1984 (G2296)"],ELLIPSOID["WGS 84",6378137,298.257223563,LENGTHUNIT["metre",1]],ENSEMBLEACCURACY[2.0]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],CS[ellipsoidal,2],AXIS["geodetic latitude (Lat)",north,ORDER[1],ANGLEUNIT["degree",0.0174532925199433]],AXIS["geodetic longitude (Lon)",east,ORDER[2],ANGLEUNIT["degree",0.0174532925199433]],USAGE[SCOPE["Horizontal component of 3D system."],AREA["World."],BBOX[-90,-180,90,180]],ID["EPSG",4326]]</wkt>
      <proj4>+proj=longlat +datum=WGS84 +no_defs</proj4>
      <srsid>3452</srsid>
      <srid>4326</srid>
      <authid>EPSG:4326</authid>
      <description>WGS 84</description>
      <projectionacronym>longlat</projectionacronym>
      <ellipsoidacronym>EPSG:7030</ellipsoidacronym>
      <geographicflag>true</geographicflag>
    </spatialrefsys>
  </crs>
  <extent>
    <spatial minx="99" maxy="58" maxx="122" dimensions="2" maxz="0" miny="48" minz="0" crs="EPSG:4326"/>
    <temporal>
      <period>
        <start></start>
        <end></end>
      </period>
    </temporal>
  </extent>
</qgis>
