<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.40.13-Bratislava">
  <identifier>C:/Job/2026/QGIS SHA Project using the USLE Lake Baikal case study/rasters/MI_GSZ2016T50P5.tif</identifier>
  <parentidentifier></parentidentifier>
  <language>eng (English)</language>
  <type>dataset</type>
  <title>General Seismic Zoning 2016 (GSZ-2016) macroseismic intensity VIII+ map for the Lake Baikal region for 5% probability of exceedance in 50 years</title>
  <abstract>Digitized copy of the latest version of the Russian General Seismic Zoning (GSZ-2016)
Macroseismic intensity fields for intensity classes VI, VII, VIII+ or larger for the Lake Baikal region for 5% probability of exceedance in 50 year.</abstract>
  <keywords vocabulary="GIS">
    <keyword>geospatial</keyword>
  </keywords>
  <keywords vocabulary="PSHA Concept">
    <keyword>General Seismic Zoning 2016 (GSZ-2016)</keyword>
  </keywords>
  <keywords vocabulary="Seismic Hazard">
    <keyword>macroseismic intensity</keyword>
  </keywords>
  <keywords vocabulary="geographicRegion">
    <keyword>Lake Baikal region</keyword>
  </keywords>
  <keywords vocabulary="gmd:topicCategory">
    <keyword>Geoscientific Information</keyword>
    <keyword>Seismic Hazard</keyword>
  </keywords>
  <contact>
    <name>Anastasiia Nekrasova</name>
    <organization>Institute of Earthquake Prediction Theory and Mathematical Geophysics RAS</organization>
    <position></position>
    <voice></voice>
    <fax></fax>
    <email>nastia$mitp.ru</email>
    <role>owner</role>
  </contact>
  <links>
    <link format="" size="" mimeType="" type="information" url="https://www.itpz-ran.ru/en/results/maps-and-databases/" description="" name="Interactive Geographic Information Projects"/>
  </links>
  <history></history>
  <dates/>
  <fees></fees>
  <constraints type="undefined 1">No restrictions for academic use. For citation, reference: Zavyalov A, Peretokin S, Danilova T, Medvedeva N, Akatova K ( 2019) General Seismic Zoning: from Maps GSZ-97 to GSZ-2016 and New-Generation Maps in the Parameters of Physical Characteristics. Seismic Instruments 55(4):445–463. https://doi.org/10.3103/S0747923919040121
</constraints>
  <license>Project Draft License 1.0 (Placeholder)</license>
  <encoding></encoding>
  <crs>
    <spatialrefsys nativeFormat="Wkt">
      <wkt>PROJCRS["WGS 84 / Pseudo-Mercator",BASEGEOGCRS["WGS 84",ENSEMBLE["World Geodetic System 1984 ensemble",MEMBER["World Geodetic System 1984 (Transit)"],MEMBER["World Geodetic System 1984 (G730)"],MEMBER["World Geodetic System 1984 (G873)"],MEMBER["World Geodetic System 1984 (G1150)"],MEMBER["World Geodetic System 1984 (G1674)"],MEMBER["World Geodetic System 1984 (G1762)"],MEMBER["World Geodetic System 1984 (G2139)"],MEMBER["World Geodetic System 1984 (G2296)"],ELLIPSOID["WGS 84",6378137,298.257223563,LENGTHUNIT["metre",1]],ENSEMBLEACCURACY[2.0]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],ID["EPSG",4326]],CONVERSION["Popular Visualisation Pseudo-Mercator",METHOD["Popular Visualisation Pseudo Mercator",ID["EPSG",1024]],PARAMETER["Latitude of natural origin",0,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8801]],PARAMETER["Longitude of natural origin",0,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8802]],PARAMETER["False easting",0,LENGTHUNIT["metre",1],ID["EPSG",8806]],PARAMETER["False northing",0,LENGTHUNIT["metre",1],ID["EPSG",8807]]],CS[Cartesian,2],AXIS["easting (X)",east,ORDER[1],LENGTHUNIT["metre",1]],AXIS["northing (Y)",north,ORDER[2],LENGTHUNIT["metre",1]],USAGE[SCOPE["Web mapping and visualisation."],AREA["World between 85.06°S and 85.06°N."],BBOX[-85.06,-180,85.06,180]],ID["EPSG",3857]]</wkt>
      <proj4>+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs</proj4>
      <srsid>3857</srsid>
      <srid>3857</srid>
      <authid>EPSG:3857</authid>
      <description>WGS 84 / Pseudo-Mercator</description>
      <projectionacronym>merc</projectionacronym>
      <ellipsoidacronym>EPSG:7030</ellipsoidacronym>
      <geographicflag>false</geographicflag>
    </spatialrefsys>
  </crs>
  <extent>
    <spatial minz="0" maxy="7967317.53500000014901161" crs="EPSG:3857" dimensions="2" miny="6106854.83490000013262033" maxx="13580977.87680000066757202" minx="11020629.5885000005364418" maxz="0"/>
    <temporal>
      <period>
        <start></start>
        <end></end>
      </period>
    </temporal>
  </extent>
</qgis>
