<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.40.13-Bratislava">
  <identifier>C:\Job\2026\QGIS SHA Project using the USLE Lake Baikal case study\data\MCM USLE.gpkg|layername=Mmax_bklABC9419dS125h6_dM0_WGS84</identifier>
  <parentidentifier></parentidentifier>
  <language>eng (English)</language>
  <type>dataset</type>
  <title>Maximum Credible Magnitude (USLE regional coefficients, BDRGS catalog data 1994-2019)</title>
  <abstract>Identification of potential seismic sources
The long-term estimates of the USLE coefficients are used for estimation of the Maximum Credible Magnitude (MCM, MMCM). expected with a p% chance of exceedance in T years following the procedures suggested in (Parvez et al. 2014). Specifically, for each ci we apply formula log10 N(M,L) = A+BM0 −M +Clog10L to calculate the expected numbers of events from magnitude ranges Mk in T-years and then find the magnitude MCM = max{Mk | T × N (Mk, L) ≥ p%}.</abstract>
  <keywords vocabulary="NDSHA concept">
    <keyword>Neo-Deterministic Seismic Hazard Assessment</keyword>
  </keywords>
  <keywords vocabulary="geographicRegion">
    <keyword>Lake Baikal region</keyword>
  </keywords>
  <keywords vocabulary="gmd:topicCategory">
    <keyword>Seismic Hazard</keyword>
  </keywords>
  <keywords vocabulary="seismichazard">
    <keyword>seismic hazard</keyword>
  </keywords>
  <contact>
    <name>Anastasiia Nekrasova</name>
    <organization>Institute of Earthquake Prediction Theory and Mathematical Geophysics RAS</organization>
    <position></position>
    <voice></voice>
    <fax></fax>
    <email>nastia$mitp.ru</email>
    <role>owner</role>
  </contact>
  <links>
    <link size="" format="" url="https://www.itpz-ran.ru/en/results/maps-and-databases/" description="" type="information" name="Interactive Geographic Information Projects" mimeType=""/>
  </links>
  <history></history>
  <dates/>
  <fees></fees>
  <constraints type="undefined 1">No restrictions for academic use. For citation, reference the Nekrasova, A., Kossobokov, V. (2023) Seismic risk assessment for the infrastructure in the regions adjacent to the Russian Federation Baikal–Amur Mainline based on the Unified Scaling Law for Earthquakes. Nat Hazards 116, 2. https://doi.org/10.1007/s11069-022-05750-9</constraints>
  <license>Project Draft License 1.0 (Placeholder)</license>
  <encoding></encoding>
  <crs>
    <spatialrefsys nativeFormat="Wkt">
      <wkt>GEOGCRS["WGS 84",ENSEMBLE["World Geodetic System 1984 ensemble",MEMBER["World Geodetic System 1984 (Transit)"],MEMBER["World Geodetic System 1984 (G730)"],MEMBER["World Geodetic System 1984 (G873)"],MEMBER["World Geodetic System 1984 (G1150)"],MEMBER["World Geodetic System 1984 (G1674)"],MEMBER["World Geodetic System 1984 (G1762)"],MEMBER["World Geodetic System 1984 (G2139)"],MEMBER["World Geodetic System 1984 (G2296)"],ELLIPSOID["WGS 84",6378137,298.257223563,LENGTHUNIT["metre",1]],ENSEMBLEACCURACY[2.0]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],CS[ellipsoidal,2],AXIS["geodetic latitude (Lat)",north,ORDER[1],ANGLEUNIT["degree",0.0174532925199433]],AXIS["geodetic longitude (Lon)",east,ORDER[2],ANGLEUNIT["degree",0.0174532925199433]],USAGE[SCOPE["Horizontal component of 3D system."],AREA["World."],BBOX[-90,-180,90,180]],ID["EPSG",4326]]</wkt>
      <proj4>+proj=longlat +datum=WGS84 +no_defs</proj4>
      <srsid>3452</srsid>
      <srid>4326</srid>
      <authid>EPSG:4326</authid>
      <description>WGS 84</description>
      <projectionacronym>longlat</projectionacronym>
      <ellipsoidacronym>EPSG:7030</ellipsoidacronym>
      <geographicflag>true</geographicflag>
    </spatialrefsys>
  </crs>
  <extent>
    <spatial miny="48" minz="0" maxx="122" maxy="58" crs="EPSG:4326" dimensions="2" minx="99" maxz="0"/>
    <temporal>
      <period>
        <start></start>
        <end></end>
      </period>
    </temporal>
  </extent>
</qgis>
