<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.40.13-Bratislava">
  <identifier>C:\Job\2026\QGIS SHA Project using the USLE Lake Baikal case study\data\MI_USLET50P10.tif</identifier>
  <parentidentifier></parentidentifier>
  <language>eng (English)</language>
  <type>dataset</type>
  <title>USLE-based macroseismic intensity map for the Lake Baikal region for 10% probability of Imax exceedance in 50 years</title>
  <abstract>Macroseismic intensity fields for intensity classes VI, VII and VIII or larger.
Use the average coefficients α = − 2.29, β = 0.57, γ = − 1.17, δ = 0.34 from (Wells and Coppersmith 1994) to describe the elliptical seismic source zones of the expected potentially potential seismic sources of magnitude 5.0 or larger. The orientation of each ellipse follows the dominant fault strike (ψ) near the epicentre. 
If no strike is defined, the plugin defaults to a circular source zone using the Shebalin (1968) model.

</abstract>
  <keywords vocabulary="GIS">
    <keyword>geospatial</keyword>
  </keywords>
  <keywords vocabulary="NDSH Concept">
    <keyword>Unified Scaling Law for Earthquakes</keyword>
  </keywords>
  <keywords vocabulary="Seismic Hazard">
    <keyword>macroseismic intensity</keyword>
  </keywords>
  <keywords vocabulary="geographicRegion">
    <keyword>Lake Baikal region</keyword>
  </keywords>
  <keywords vocabulary="gmd:topicCategory">
    <keyword>Seismic Hazard</keyword>
  </keywords>
  <contact>
    <name>Anastasiia Nekrasova</name>
    <organization>Institute of Earthquake Prediction Theory and Mathematical Geophysics RAS</organization>
    <position></position>
    <voice></voice>
    <fax></fax>
    <email>nastia$mitp.ru</email>
    <role>owner</role>
  </contact>
  <links>
    <link size="" format="" url="https://www.itpz-ran.ru/en/results/maps-and-databases/" description="" type="information" name="Interactive Geographic Information Projects" mimeType=""/>
  </links>
  <history></history>
  <dates/>
  <fees></fees>
  <constraints type="undefined 1">No restrictions for academic use. For citation, reference the Nekrasova, A., Kossobokov, V. (2023) Seismic risk assessment for the infrastructure in the regions adjacent to the Russian Federation Baikal–Amur Mainline based on the Unified Scaling Law for Earthquakes. Nat Hazards 116, 2. https://doi.org/10.1007/s11069-022-05750-9</constraints>
  <license>Project Draft License 1.0 (Placeholder)</license>
  <encoding></encoding>
  <crs>
    <spatialrefsys nativeFormat="Wkt">
      <wkt>PROJCRS["WGS 84 / Pseudo-Mercator",BASEGEOGCRS["WGS 84",ENSEMBLE["World Geodetic System 1984 ensemble",MEMBER["World Geodetic System 1984 (Transit)"],MEMBER["World Geodetic System 1984 (G730)"],MEMBER["World Geodetic System 1984 (G873)"],MEMBER["World Geodetic System 1984 (G1150)"],MEMBER["World Geodetic System 1984 (G1674)"],MEMBER["World Geodetic System 1984 (G1762)"],MEMBER["World Geodetic System 1984 (G2139)"],MEMBER["World Geodetic System 1984 (G2296)"],ELLIPSOID["WGS 84",6378137,298.257223563,LENGTHUNIT["metre",1]],ENSEMBLEACCURACY[2.0]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],ID["EPSG",4326]],CONVERSION["Popular Visualisation Pseudo-Mercator",METHOD["Popular Visualisation Pseudo Mercator",ID["EPSG",1024]],PARAMETER["Latitude of natural origin",0,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8801]],PARAMETER["Longitude of natural origin",0,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8802]],PARAMETER["False easting",0,LENGTHUNIT["metre",1],ID["EPSG",8806]],PARAMETER["False northing",0,LENGTHUNIT["metre",1],ID["EPSG",8807]]],CS[Cartesian,2],AXIS["easting (X)",east,ORDER[1],LENGTHUNIT["metre",1]],AXIS["northing (Y)",north,ORDER[2],LENGTHUNIT["metre",1]],USAGE[SCOPE["Web mapping and visualisation."],AREA["World between 85.06°S and 85.06°N."],BBOX[-85.06,-180,85.06,180]],ID["EPSG",3857]]</wkt>
      <proj4>+proj=merc +a=6378137 +b=6378137 +lat_ts=0 +lon_0=0 +x_0=0 +y_0=0 +k=1 +units=m +nadgrids=@null +wktext +no_defs</proj4>
      <srsid>3857</srsid>
      <srid>3857</srid>
      <authid>EPSG:3857</authid>
      <description>WGS 84 / Pseudo-Mercator</description>
      <projectionacronym>merc</projectionacronym>
      <ellipsoidacronym>EPSG:7030</ellipsoidacronym>
      <geographicflag>false</geographicflag>
    </spatialrefsys>
  </crs>
  <extent>
    <spatial miny="6106854.83490000013262033" minz="0" maxx="13580977.87680000066757202" maxy="7967317.53500000014901161" crs="EPSG:3857" dimensions="2" minx="11020629.5885000005364418" maxz="0"/>
    <temporal>
      <period>
        <start></start>
        <end></end>
      </period>
    </temporal>
  </extent>
</qgis>
